TIFFcolor — LibTIFF 4.7.1 documentation

# TIFFcolor

## Synopsis

    #include <tiffio.h>

int TIFFYCbCrToRGBInit(TIFFYCbCrToRGB *ycbcr, float *luma, float *refBlackWhite)

void TIFFYCbCrtoRGB(TIFFYCbCrToRGB *ycbcr, uint32_t Y, int32_t Cb, int32_t Cr, uint32_t *R, uint32_t *G, uint32_t *B)

int TIFFCIELabToRGBInit(TIFFCIELabToRGB *cielab, const TIFFDisplay *displayw, float *refWhite)

void TIFFCIELabToXYZ(TIFFCIELabToRGB *cielab, uint32_t L, int32_t a, int32_t b, float *X, float *Y, float *Z)

void TIFFXYZToRGB(TIFFCIELabToRGB *cielab, float X, float Y, float Z, uint32_t *R, uint32_t *G, uint32_t *B)

## Description

TIFF supports several color spaces for images stored in that format. There is usually a problem of application to handle the data properly and convert between different colorspaces for displaying and printing purposes. To simplify this task `libtiff` implements several color conversion routines itself. In particular, these routines used in the TIFFRGBAImage interface.

`TIFFYCbCrToRGBInit()` used to initialize YCbCr to RGB conversion state.

Note

The calling program is responsible for allocating and releasing the required buffer for the structure `TIFFYCbCrToRGB` and its required tables, pointed to by ycbcr. The pointers to these tables are stored in the structure `TIFFYCbCrToRGB`, which is located at the beginning of that buffer. Thus, this memory has to be allocated as shown in the example below.

`TIFFYCbCrToRGB` is defined in `tiffio.h` as:

    typedef struct {                /* YCbCr->RGB support */
            TIFFRGBValue* clamptab; /* range clamping table */
            int*          Cr_r_tab;
            int*          Cb_b_tab;
            int32_t*      Cr_g_tab;
            int32_t*      Cb_g_tab;
            int32_t*      Y_tab;
    } TIFFYCbCrToRGB;

luma is a float array of three values representing proportions of the red, green and blue in luminance, Y (see section 21 of the TIFF 6.0 specification, where YCbCr images are discussed). `TIFFTAG_YCBCRCOEFFICIENTS` hold these values in TIFF file. refBlackWhite is a float array of 6 values which specifies a pair of headroom and footroom image data values (codes) for each image component (see section 20 of the TIFF 6.0 specification where the colorimetry fields are discussed). `TIFFTAG_REFERENCEBLACKWHITE` is responsible for storing these values in TIFF file. The following code snippet should help to understand the the technique:

    float *luma, *refBlackWhite;
    uint16_t hs, vs;

    /* Initialize structures */
    TIFFYCbCrToRGB *ycbcr = (TIFFYCbCrToRGB*)
        _TIFFmalloc(TIFFroundup(sizeof(TIFFYCbCrToRGB), sizeof(long))
            + 4*256*sizeof(TIFFRGBValue)
            + 2*256*sizeof(int)
            + 3*256*sizeof(int32_t));
    if (ycbcr == NULL) {
        TIFFError("YCbCr->RGB",
        "No space for YCbCr->RGB conversion state");
        exit(0);
    }

    TIFFGetFieldDefaulted(tif, TIFFTAG_YCBCRCOEFFICIENTS, &luma);
    TIFFGetFieldDefaulted(tif, TIFFTAG_REFERENCEBLACKWHITE, &refBlackWhite);
    if (TIFFYCbCrToRGBInit(ycbcr, luma, refBlackWhite) < 0) {
        exit(0);
    }

    /* Start conversion */
    uint32_t r, g, b;
    uint32_t Y;
    int32_t Cb, Cr;

    for each pixel in image {
        TIFFYCbCrtoRGB(img->ycbcr, Y, Cb, Cr, &r, &g, &b);
    }

    /* Free state structure */
    _TIFFfree(ycbcr);

`TIFFCIELabToRGBInit()` initializes the CIE L*a*b* 1976 to RGB conversion state. `TIFFCIELabToRGB` is defined as:

    #define CIELABTORGB_TABLE_RANGE 1500

    typedef struct {                                /* CIE Lab 1976->RGB support */
        int      range;                             /* Size of conversion table */
        float    rstep, gstep, bstep;
        float    X0, Y0, Z0;                        /* Reference white point */
        TIFFDisplay display;
        float    Yr2r[CIELABTORGB_TABLE_RANGE + 1]; /* Conversion of Yr to r */
        float    Yg2g[CIELABTORGB_TABLE_RANGE + 1]; /* Conversion of Yg to g */
        float    Yb2b[CIELABTORGB_TABLE_RANGE + 1]; /* Conversion of Yb to b */
    } TIFFCIELabToRGB;

display is a display device description, declared as:

    typedef struct {
        float d_mat[3][3]; /* XYZ -> luminance matrix */
        float d_YCR;       /* Light o/p for reference white */
        float d_YCG;
        float d_YCB;
        uint32_t d_Vrwr;   /* Pixel values for ref. white */
        uint32_t d_Vrwg;
        uint32_t d_Vrwb;
        float d_Y0R;       /* Residual light for black pixel */
        float d_Y0G;
        float d_Y0B;
        float d_gammaR;    /* Gamma values for the three guns */
        float d_gammaG;
        float d_gammaB;
    } TIFFDisplay;

For example, one can use sRGB device, which has the following parameters:

    TIFFDisplay display_sRGB = {
        {   /* XYZ -> luminance matrix */
            {  3.2410F, -1.5374F, -0.4986F },
            {  -0.9692F, 1.8760F, 0.0416F },
            {  0.0556F, -0.2040F, 1.0570F }
        },
        100.0F, 100.0F, 100.0F, /* Light o/p for reference white */
        255, 255, 255,          /* Pixel values for ref. white */
        1.0F, 1.0F, 1.0F,       /* Residual light o/p for black pixel */
        2.4F, 2.4F, 2.4F,       /* Gamma values for the three guns */
    };

refWhite is a color temperature of the reference white. The `TIFFTAG_WHITEPOINT` contains the chromaticity of the white point of the image from where the reference white can be calculated using following formulae:

    refWhite_Y = 100.0

    refWhite_X = whitePoint_x / whitePoint_y * refWhite_Y

    refWhite_Z = (1.0 - whitePoint_x - whitePoint_y) / whitePoint_y * refWhite_X

The conversion itself performed in two steps: at the first one we will convert CIE L*a*b* 1976 to CIE XYZ using the `TIFFCIELabToXYZ()` routine, and at the second step we will convert CIE XYZ to RGB using `TIFFXYZToRGB()`. Look at the code sample below:

    float   *whitePoint;
    float   refWhite[3];

    /* Initialize structures */
    img->cielab = (TIFFCIELabToRGB *)
        _TIFFmalloc(sizeof(TIFFCIELabToRGB));
    if (!cielab) {
        TIFFError("CIE L*a*b*->RGB",
            "No space for CIE L*a*b*->RGB conversion state.");
        exit(0);
    }

    TIFFGetFieldDefaulted(tif, TIFFTAG_WHITEPOINT, &whitePoint);
    refWhite[1] = 100.0F;
    refWhite[0] = whitePoint[0] / whitePoint[1] * refWhite[1];
    refWhite[2] = (1.0F - whitePoint[0] - whitePoint[1])
        / whitePoint[1] * refWhite[1];
    if (TIFFCIELabToRGBInit(cielab, &display_sRGB, refWhite) < 0) {
        TIFFError("CIE L*a*b*->RGB",
            "Failed to initialize CIE L*a*b*->RGB conversion state.");
        _TIFFfree(cielab);
        exit(0);
    }

    /* Now we can start to convert */
    uint32_t r, g, b;
    uint32_t L;
    int32_t a, b;
    float X, Y, Z;

    for each pixel in image {
        TIFFCIELabToXYZ(cielab, L, a, b, &X, &Y, &Z);
        TIFFXYZToRGB(cielab, X, Y, Z, &r, &g, &b);
    }

    /* Don't forget to free the state structure */
    _TIFFfree(cielab);

## See also

TIFFRGBAImage (3tiff), libtiff (3tiff)